# Static Call Analysis for
USCALECAN (?C_STARTUP)

Created from: LX51 LINKER/LOCATER V4.10a
Creation time: 05/07/2007 23:55:10

## ?PR?MAIN?MAIN (C:000035H - C:000044H)

Maximum Stack: Bottom=8 Bytes (?PR?MAIN_VINIT?MAIN)

Calls to:

- ?PR?_ADC_VSTARTSEQREQCHNUM?ADC
- ?PR?ADC_VSEQSOFTTRIG?ADC
- ?PR?MAIN_VINIT?MAIN

## ?PR?SHINT_VIXINTR11ISR?SHARED_INT (C:000331H - C:0003FBH)

Maximum Stack: Bottom=24 Bytes (?PR?_CAN_VTRANSMIT?CAN)

Calls to:

- ?PR?_CAN_VTRANSMIT?CAN
- ?PR?_UART_VSENDDATA8?UART
- ?PR?ADC_UWGETRESULTDATA0?ADC

## ?PR?MAIN_VINIT?MAIN (C:000003H - C:000024H)

Maximum Stack: Bottom=6 Bytes (?PR?CAN_VINIT?CAN) Top=2 Bytes (?PR?MAIN?MAIN)

Calls to:

- ?PR?ADC_VINIT?ADC
- ?PR?CAN_VINIT?CAN
- ?PR?CC6_VINIT?CC6
- ?PR?SHINT_VINIT?SHARED_INT
- ?PR?UART_VINIT?UART

Called from:

- ?PR?MAIN?MAIN

## ?PR?CC6_VINIT?CC6 (C:0000B1H - C:000129H)

Maximum Stack: Top=4 Bytes (?PR?MAIN_VINIT?MAIN)

Called from:

- ?PR?MAIN_VINIT?MAIN

## ?PR?SHINT_VINIT?SHARED_INT (C:000025H - C:000028H)

Maximum Stack: Top=4 Bytes (?PR?MAIN_VINIT?MAIN)

Called from:

- ?PR?MAIN_VINIT?MAIN

## ?PR?ADC_VINIT?ADC (C:0002F4H - C:000330H)

Maximum Stack: Top=4 Bytes (?PR?MAIN_VINIT?MAIN)

Called from:

- ?PR?MAIN_VINIT?MAIN

## ?PR?ADC_VSEQSOFTTRIG?ADC (C:0002A9H - C:0002B2H)

Maximum Stack: Top=2 Bytes (?PR?MAIN?MAIN)

Called from:

- ?PR?MAIN?MAIN

## ?PR?_ADC_VSTARTSEQREQCHNUM?ADC (C:0002D1H - C:0002F3H)

Maximum Stack: Top=2 Bytes (?PR?MAIN?MAIN)

Called from:

- ?PR?MAIN?MAIN

## ?PR?ADC_UWGETRESULTDATA0?ADC (C:0003FCH - C:00040CH)

Maximum Stack: Top=18 Bytes (?PR?SHINT_VIXINTR11ISR?SHARED_INT)

Called from:

- ?PR?SHINT_VIXINTR11ISR?SHARED_INT

## ?PR?UART_VINIT?UART (C:0002B3H - C:0002D0H)

Maximum Stack: Top=4 Bytes (?PR?MAIN_VINIT?MAIN)

Called from:

- ?PR?MAIN_VINIT?MAIN

## ?PR?_UART_VSENDDATA8?UART (C:000029H - C:00002DH)

Maximum Stack: Top=18 Bytes (?PR?SHINT_VIXINTR11ISR?SHARED_INT)

Called from:

- ?PR?SHINT_VIXINTR11ISR?SHARED_INT

## ?PR?CAN_VINIT?CAN (C:00012AH - C:00025FH)

Maximum Stack: Bottom=4 Bytes (?PR?_CAN_VSETLISTCOMMAND?CAN) Top=4 Bytes (?PR?MAIN_VINIT?MAIN)

Calls to:

- ?PR?_CAN_VSETLISTCOMMAND?CAN
- ?PR?_CAN_VWRITEAMDATA?CAN

Called from:

- ?PR?MAIN_VINIT?MAIN

## ?PR?_CAN_VWRITEAMDATA?CAN (C:000260H - C:000298H)

Maximum Stack: Top=8 Bytes (?PR?_CAN_VSETLISTCOMMAND?CAN)

Called from:

- ?PR?_CAN_VSETLISTCOMMAND?CAN
- ?PR?CAN_VINIT?CAN

## ?PR?_CAN_VSETLISTCOMMAND?CAN (C:000299H - C:0002A8H)

Maximum Stack: Bottom=2 Bytes (?PR?_CAN_VWRITEAMDATA?CAN) Top=6 Bytes (?PR?CAN_VINIT?CAN)

Calls to:

- ?PR?_CAN_VWRITEAMDATA?CAN

Called from:

- ?PR?CAN_VINIT?CAN

## ?PR?_CAN_VTRANSMIT?CAN (C:00040DH - C:00044DH)

Maximum Stack: Top=18 Bytes (?PR?SHINT_VIXINTR11ISR?SHARED_INT)

Called from:

- ?PR?SHINT_VIXINTR11ISR?SHARED_INT