# Static Call Analysis for
USCALEPWM (?C_STARTUP)

Created from: LX51 LINKER/LOCATER V4.10a
Creation time: 05/10/2007 11:11:44

## ?PR?MAIN?MAIN (C:00007DH - C:00008CH)

Maximum Stack: Bottom=4 Bytes (?PR?MAIN_VINIT?MAIN)

Calls to:

- ?PR?_ADC_VSTARTSEQREQCHNUM?ADC
- ?PR?ADC_VSEQSOFTTRIG?ADC
- ?PR?MAIN_VINIT?MAIN

## ?PR?SHINT_VIXINTR11ISR?SHARED_INT (C:00018EH - C:00022EH)

Maximum Stack: Bottom=18 Bytes (?PR?ADC_UWGETRESULTDATA0?ADC)

Calls to:

- ?PR?_UART_VSENDDATA8?UART
- ?PR?ADC_UWGETRESULTDATA0?ADC

## ?PR?MAIN_VINIT?MAIN (C:00005DH - C:00007CH)

Maximum Stack: Bottom=2 Bytes (?PR?UART_VINIT?UART) Top=2 Bytes (?PR?MAIN?MAIN)

Calls to:

- ?PR?ADC_VINIT?ADC
- ?PR?CC6_VINIT?CC6
- ?PR?SHINT_VINIT?SHARED_INT
- ?PR?UART_VINIT?UART

Called from:

- ?PR?MAIN?MAIN

## ?PR?CC6_VINIT?CC6 (C:000115H - C:00018DH)

Maximum Stack: Top=4 Bytes (?PR?MAIN_VINIT?MAIN)

Called from:

- ?PR?MAIN_VINIT?MAIN

## ?PR?SHINT_VINIT?SHARED_INT (C:000057H - C:00005AH)

Maximum Stack: Top=4 Bytes (?PR?MAIN_VINIT?MAIN)

Called from:

- ?PR?MAIN_VINIT?MAIN

## ?PR?ADC_VINIT?ADC (C:0000D8H - C:000114H)

Maximum Stack: Top=4 Bytes (?PR?MAIN_VINIT?MAIN)

Called from:

- ?PR?MAIN_VINIT?MAIN

## ?PR?ADC_VSEQSOFTTRIG?ADC (C:00008DH - C:000096H)

Maximum Stack: Top=2 Bytes (?PR?MAIN?MAIN)

Called from:

- ?PR?MAIN?MAIN

## ?PR?_ADC_VSTARTSEQREQCHNUM?ADC (C:0000B5H - C:0000D7H)

Maximum Stack: Top=2 Bytes (?PR?MAIN?MAIN)

Called from:

- ?PR?MAIN?MAIN

## ?PR?ADC_UWGETRESULTDATA0?ADC (C:000234H - C:000244H)

Maximum Stack: Top=18 Bytes (?PR?SHINT_VIXINTR11ISR?SHARED_INT)

Called from:

- ?PR?SHINT_VIXINTR11ISR?SHARED_INT

## ?PR?UART_VINIT?UART (C:000097H - C:0000B4H)

Maximum Stack: Top=4 Bytes (?PR?MAIN_VINIT?MAIN)

Called from:

- ?PR?MAIN_VINIT?MAIN

## ?PR?_UART_VSENDDATA8?UART (C:00022FH - C:000233H)

Maximum Stack: Top=18 Bytes (?PR?SHINT_VIXINTR11ISR?SHARED_INT)

Called from:

- ?PR?SHINT_VIXINTR11ISR?SHARED_INT